3GPP TR 38.814 V15.0.0 (2018-06)

Technical Report

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

New frequency range for NR (4.4-5.0 GHz)

(Release 15)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2018, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 4

1 Scope 5

2 References 5

3 Definitions, symbols and abbreviations 5

3.1 Definitions 5

3.2 Symbols 5

3.3 Abbreviations 5

4 Background 6

5 NR Frequency band definition 6

6 Channel numbering and channel bandwidth 6

7 NR band 4.4-5.0 GHz issues 7

7.1 UE specific 7

7.1.1 Transmitter characteristics 7

7.1.1.1 UE maximum output power 7

7.1.2 Receiver characteristics 8

7.1.2.1 Reference sensitivity 8

7.1.2.2 Blocking 8

7.1.2.2.1 Out-of-band blocking 8

8 Required changes to NR, E-UTRA, UTRA and MSR specifications 9

Annex A: Change history 10

# Foreword

This Technical Report has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document is a technical report for Work Item on New Radio (NR) Access Technology, covering the new frequency range between 4.4 – 5.0 GHz for NR.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

FInterferer Frequency of the interferer

FDL\_low The lowest frequency of the downlink operating band

FDL\_high The highest frequency of the downlink operating band

PInterferer Modulated mean power of the interferer

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

BW Bandwidth

NR New Radio

RF Radio Frequency

SCS Sub-Carrier Spacing

TDD Time division Duplex

UE User Equipment

# 4 Background

Recently, two countries such as Japan and China have announced their “5G” spectrum strategies and roadmaps for the frequency range between 4.4-5.0 GHz to deploy commercial stems for NR as follows.



Figure 4-1: NR spectrum plans in the range between 4.4 – 5.0 GHz

# 5 NR Frequency band definition

Considering the spectrum plans in each country described in the section 4, the band plan for 4.4 – 5.0 GHz frequency range is decided as shown in Figure 5-1.



Figure 5-1: Band definition in the frequency range between 4.4 – 5.0 GHz

# 6 Channel numbering and channel bandwidth

Band numbering for the range and applicable duplex mode for 4.4 – 5.0 GHz are provided in Table 6-1.

Table 6-1: New NR band in the frequency range between 4.4 – 5.0 GHz

|  |  |  |  |
| --- | --- | --- | --- |
| **Band number** | **UL** | **DL** | **Duplex mode** |
| n79 | 4.4 – 5.0 GHz | 4.4 – 5.0 GHz | TDD |

Available channel bandwidths for n79 are summarized below.

Table 6-2: Channel Bandwidths for n79

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR band / SCS / UE Channel bandwidth | | | | | | | | | | | | |
| NR Band | SCS  kHz | 5 MHz | 101,2 MHz | 152 MHz | 202 MHz | 252 MHz | 30 MHz | 40 MHz | 50 MHz | 60 MHz | 80 MHz | 100 MHz |
| n79 | 15 |  |  |  |  |  |  | Yes | Yes |  |  |  |
| 30 |  |  |  |  |  |  | Yes | Yes | Yes | Yes | Yes |
| 60 |  |  |  |  |  |  | Yes | Yes | Yes | Yes | Yes |
| NOTE 1: 90% spectrum utilization may not be achieved for 30kHz SCS.  NOTE 2: 90% spectrum utilization may not be achieved for 60kHz SCS.  NOTE 3: This UE channel bandwidth is applicable only to downlink. | | | | | | | | | | | | |

# 7 NR band 4.4-5.0 GHz issues

## 7.1 UE specific

### 7.1.1 Transmitter characteristics

#### 7.1.1.1 UE maximum output power


The MOP requirements for Band 42 and 43 single-carrier were specified as 23 dBm +2/-3 dB for power class 3 based on simulation results shown in Table 7.1.1.1-1 in August 2011.

Table 7.1.1.1-1: Simulation results for combined Band 42 and Band 43 filter [R4-114656]

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Bandwidth | Max IL (corner) | 2f0 rejection | 2.7 GHz rejection |
| Design 7 | 400 MHz | 1.9 | 20 dB | 30 dB |
| Design 8 | 400 MHz | 2.3 | 15 dB | 10 dB |
| Design 9 | 400 MHz | 2.0 | 20 dB | 15 dB |

BPFs for Band n79 are provided in Table 7.1.1.1-2 and 7.1.1.1-3.

Table 7.1.1.1-2: Simulation results for combined Band 42 and Band 43 filter [R4-114656]



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| F [GHz] | 4.4 | 4.8 | 4.99 | 5.0 |
| IL +25C [dB] | 0.88 | 0.60 | 0.59 | 0.59 |
| IL ETC -40~+90C [dB] | 1.1 | 0.8 | 0.80 | 0.80 |

Table 7.1.1.1-3: Simulation results for combined Band 42 and Band 43 filter [R4-114656]

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | typ IL [dB] | | | worst IL [dB] | | | Attenuation [dB] | | | | | |
| frequencies [GHz] | 4.4 | 4.8 | 5 | 4.4 | 4.8 | 5 | 2.3-2.69 | 0.617-2.2 | 3.3-4.2 | 3.3-3.8 | 5.15-5.925 | 5.250-5.925 |
| n79 filter TR | 2.3 | 1 | 2.3 | 2.5 | 1.2 | 2.5 | >35 | >25 | >15 | >15 | >40 | >40 |
| comment | 4.4-4.5GHz range must demonstrate coexistence with altimeter band for China | | | | | | | | | | | |
| improved rejection in WiFi band | | | | | | | | | | | |

From these tables, no significant filter IL degradation for Band n79 can be seen compared to that of Band 42 and 43 at ETC condition. Therefore, MOP for Band n79 should be aligned with those of Band 42 and 43 at least.

Agreement: MOP for Band n79 is to be 23 dBm +2/-3 dB

### 7.1.2 Receiver characteristics

#### 7.1.2.1 Reference sensitivity

With the same investigation as UE maximum output power described in 7.1.1.1, no significant filter IL degradation for Band n79 can be seen compared to that of Band 42 and 43 at ETC condition. In addition, from LNA perspective, the fractional bandwidth of Band n79 pass-band is 12.8 % which is smaller than that of Band n78 (14.1 %). Hence, NF of Band n79 shouldn’t be higher than that of Band n78. Therefore, reference sensitivity for Band n79 should also be aligned with those of Band n78 at least.

Agreement: REFSENS for Band n79 should be 1 dB larger than that of bands which have NR smallest sensitivity (less RF challenges) such as Band n1.

Table 7.1.2.1-1: Reference sensitivity for Band n79

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | SCS kHz | 40 | 50 | 60 | 80 | 100 | Duplex Mode |
| MHz | MHz | MHz | MHz | MHz |
| (dBm) | (dBm) | (dBm) | (dBm) | (dBm) |
| n79 | 15 | -89.6 | -88.6 |  |  |  | TDD |
| 30 | -89.7 | -88.7 | -87.9 | -86.6 | -85.6 |
| 60 | -89.9 | -88.8 | -88.0 | -86.7 | -85.7 |

#### 7.1.2.2 Blocking

##### 7.1.2.2.1 Out-of-band blocking

Based on filter performance shown in Table 7.1.1.1-1 and 7.1.1.1-2, out-of-band blocking requirement needs to be optimized as with LTE band 42 and 43 as below.

Table 7.1.2.2.1-1: Out-of-band blocking parameters for Band n79

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Rx Parameter** | **Units** | **Channel bandwidth** | | | | |
| **40 MHz** | **50 MHz** | **60 MHz** | **80 MHz** | **100 MHz** |
| Power in Transmission Bandwidth Configuration | dBm | REFSENS + channel bandwidth specific value below | | | | |
| 9 | 9 | 9 | 9 | 9 |
| NOTE 1: The transmitter shall be set to 4dB below PCMAX\_L at the minimum uplink configuration specified TBD with PCMAX\_L as defined in subclause 6.2.5.  NOTE 2: Reference measurement channel is TBD  NOTE 3: The REFSENS power level is TBD | | | | | | |

Table 7.1.2.2.1-2: Out of band blocking for Band n79

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **NR band** | **Parameter** | **Units** | **Frequency** | | |
| **Range 1** | **Range 2** | **Range 3** |
| PInterferer | dBm | -44 | -30 | -15 |
| n79 (NOTE 2) | FInterferer (CW) | MHz | N/A | -150 < f – FDL\_low ≤ -MIN(150,3CBW)  or  MIN(150,3CBW) ≤ f – FDL\_high < 150 | 1 ≤ f ≤ FDL\_low – MIN(150,3CBW)  or  FDL\_high + MIN(150,3CBW) ≤ f ≤ 12750 |
| NOTE 1: CBW denotes the channel bandwidth of the wanted signal  NOTE 2: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm, for FInterferer > 3650 MHz and FInterferer < 5750 MHz. For CBW equal or larger than 50 MHz, the requirement for Range 2 is not applicable and Range 3 applies from the frequency offset of 3\*CBW from the band edge. | | | | | |

# 8 Required changes to NR, E-UTRA, UTRA and MSR specifications

No changes identified.

Annex A:  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2017-08 | RAN4#84 | R4-1708172 |  |  |  | Skeleton TR 38.814 | 0.0.1 |
| 2018-01 | ARN4AH-1801 | R4-1800831 |  |  |  | draft TR 38.814 (NR 4.4-5.0GHz band) | 0.1.0 |
| 2018-03 | RAN#79 | RP-180334 |  |  |  | v1.0.0 presented to plenary for information | 1.0.0 |
| 2018-06 | RAN#80 |  |  |  |  | v2.0.0 presented to plenary for approval | 2.0.0 |
| 2018-06 | RAN#80 |  |  |  |  | Approved by plenary – Rel-15 spec under change control | 15.0.0 |